From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Mon, 16 Mar 2020 21:35:01 +0800
Subject: [PATCH] drm: panel: add Xingbangda XBD599 panel

Xingbangda XBD599 is a 5.99" 720x1440 MIPI-DSI IPS LCD panel made by
Xingbangda, which is used on PinePhone final assembled phones.

Add support for it.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 drivers/gpu/drm/panel/Kconfig                 |   9 +
 drivers/gpu/drm/panel/Makefile                |   1 +
 .../gpu/drm/panel/panel-xingbangda-xbd599.c   | 366 ++++++++++++++++++
 3 files changed, 376 insertions(+)
 create mode 100644 drivers/gpu/drm/panel/panel-xingbangda-xbd599.c

diff --git a/drivers/gpu/drm/panel/Kconfig b/drivers/gpu/drm/panel/Kconfig
index de2f2a452be5..3ce658de416b 100644
--- a/drivers/gpu/drm/panel/Kconfig
+++ b/drivers/gpu/drm/panel/Kconfig
@@ -462,6 +462,15 @@ config DRM_PANEL_VISIONOX_RM69299
 	  Say Y here if you want to enable support for Visionox
 	  RM69299  DSI Video Mode panel.

+config DRM_PANEL_XINGBANGDA_XBD599
+	tristate "Xingbangda XBD599 panel"
+	depends on OF
+	depends on DRM_MIPI_DSI
+	depends on BACKLIGHT_CLASS_DEVICE
+	help
+	  Say Y here if you want to enable support for the Xingbangda XBD599
+	  MIPI DSI Video Mode panel.
+
 config DRM_PANEL_XINPENG_XPP055C272
 	tristate "Xinpeng XPP055C272 panel driver"
 	depends on OF
diff --git a/drivers/gpu/drm/panel/Makefile b/drivers/gpu/drm/panel/Makefile
index e45ceac6286f..bd10617430ec 100644
--- a/drivers/gpu/drm/panel/Makefile
+++ b/drivers/gpu/drm/panel/Makefile
@@ -49,4 +49,5 @@ obj-$(CONFIG_DRM_PANEL_TPO_TD043MTEA1) += panel-tpo-td043mtea1.o
 obj-$(CONFIG_DRM_PANEL_TPO_TPG110) += panel-tpo-tpg110.o
 obj-$(CONFIG_DRM_PANEL_TRULY_NT35597_WQXGA) += panel-truly-nt35597.o
 obj-$(CONFIG_DRM_PANEL_VISIONOX_RM69299) += panel-visionox-rm69299.o
+obj-$(CONFIG_DRM_PANEL_XINGBANGDA_XBD599) += panel-xingbangda-xbd599.o
 obj-$(CONFIG_DRM_PANEL_XINPENG_XPP055C272) += panel-xinpeng-xpp055c272.o
diff --git a/drivers/gpu/drm/panel/panel-xingbangda-xbd599.c b/drivers/gpu/drm/panel/panel-xingbangda-xbd599.c
new file mode 100644
index 000000000000..b483f96ee1db
--- /dev/null
+++ b/drivers/gpu/drm/panel/panel-xingbangda-xbd599.c
@@ -0,0 +1,366 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Xingbangda XBD599 MIPI-DSI panel driver
+ *
+ * Copyright (C) 2019-2020 Icenowy Zheng <icenowy@aosc.io>
+ *
+ * Based on panel-rocktech-jh057n00900.c, which is:
+ *   Copyright (C) Purism SPC 2019
+ */
+
+#include <linux/delay.h>
+#include <linux/gpio/consumer.h>
+#include <linux/mod_devicetable.h>
+#include <linux/module.h>
+#include <linux/of_device.h>
+#include <linux/regulator/consumer.h>
+
+#include <drm/drm_mipi_dsi.h>
+#include <drm/drm_modes.h>
+#include <drm/drm_panel.h>
+#include <drm/drm_print.h>
+
+/* Manufacturer specific Commands send via DSI */
+#define ST7703_CMD_ALL_PIXEL_OFF 0x22
+#define ST7703_CMD_ALL_PIXEL_ON	 0x23
+#define ST7703_CMD_SETDISP	 0xB2
+#define ST7703_CMD_SETRGBIF	 0xB3
+#define ST7703_CMD_SETCYC	 0xB4
+#define ST7703_CMD_SETBGP	 0xB5
+#define ST7703_CMD_SETVCOM	 0xB6
+#define ST7703_CMD_SETOTP	 0xB7
+#define ST7703_CMD_SETPOWER_EXT	 0xB8
+#define ST7703_CMD_SETEXTC	 0xB9
+#define ST7703_CMD_SETMIPI	 0xBA
+#define ST7703_CMD_SETVDC	 0xBC
+#define ST7703_CMD_SETSCR	 0xC0
+#define ST7703_CMD_SETPOWER	 0xC1
+#define ST7703_CMD_UNK_C6	 0xC6
+#define ST7703_CMD_SETPANEL	 0xCC
+#define ST7703_CMD_SETGAMMA	 0xE0
+#define ST7703_CMD_SETEQ	 0xE3
+#define ST7703_CMD_SETGIP1	 0xE9
+#define ST7703_CMD_SETGIP2	 0xEA
+
+static const char * const regulator_names[] = {
+	"iovcc",
+	"vcc",
+};
+
+struct xbd599 {
+	struct device *dev;
+	struct drm_panel panel;
+	struct gpio_desc *reset_gpio;
+	struct regulator_bulk_data supplies[ARRAY_SIZE(regulator_names)];
+	bool prepared;
+};
+
+static inline struct xbd599 *panel_to_xbd599(struct drm_panel *panel)
+{
+	return container_of(panel, struct xbd599, panel);
+}
+
+#define dsi_dcs_write_seq(dsi, cmd, seq...) do {			\
+		static const u8 d[] = { seq };				\
+		int ret;						\
+		ret = mipi_dsi_dcs_write(dsi, cmd, d, ARRAY_SIZE(d));	\
+		if (ret < 0)						\
+			return ret;					\
+	} while (0)
+
+static int xbd599_init_sequence(struct xbd599 *ctx)
+{
+	struct mipi_dsi_device *dsi = to_mipi_dsi_device(ctx->dev);
+	struct device *dev = ctx->dev;
+	int ret;
+
+	/*
+	 * Init sequence was supplied by the panel vendor.
+	 */
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETEXTC,
+			  0xF1, 0x12, 0x83);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETMIPI,
+			  0x33, 0x81, 0x05, 0xF9, 0x0E, 0x0E, 0x20, 0x00,
+			  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x44, 0x25,
+			  0x00, 0x91, 0x0a, 0x00, 0x00, 0x02, 0x4F, 0x11,
+			  0x00, 0x00, 0x37);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETPOWER_EXT,
+			  0x25, 0x22, 0x20, 0x03);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETRGBIF,
+			  0x10, 0x10, 0x05, 0x05, 0x03, 0xFF, 0x00, 0x00,
+			  0x00, 0x00);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETSCR,
+			  0x73, 0x73, 0x50, 0x50, 0x00, 0xC0, 0x08, 0x70,
+			  0x00);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETVDC, 0x4E);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETPANEL, 0x0B);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETCYC, 0x80);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETDISP, 0xF0, 0x12, 0xF0);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETEQ,
+			  0x00, 0x00, 0x0B, 0x0B, 0x10, 0x10, 0x00, 0x00,
+			  0x00, 0x00, 0xFF, 0x00, 0xC0, 0x10);
+	dsi_dcs_write_seq(dsi, 0xC6, 0x01, 0x00, 0xFF, 0xFF, 0x00);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETPOWER,
+			  0x74, 0x00, 0x32, 0x32, 0x77, 0xF1, 0xFF, 0xFF,
+			  0xCC, 0xCC, 0x77, 0x77);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETBGP, 0x07, 0x07);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETVCOM, 0x2C, 0x2C);
+	dsi_dcs_write_seq(dsi, 0xBF, 0x02, 0x11, 0x00);
+
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETGIP1,
+			  0x82, 0x10, 0x06, 0x05, 0xA2, 0x0A, 0xA5, 0x12,
+			  0x31, 0x23, 0x37, 0x83, 0x04, 0xBC, 0x27, 0x38,
+			  0x0C, 0x00, 0x03, 0x00, 0x00, 0x00, 0x0C, 0x00,
+			  0x03, 0x00, 0x00, 0x00, 0x75, 0x75, 0x31, 0x88,
+			  0x88, 0x88, 0x88, 0x88, 0x88, 0x13, 0x88, 0x64,
+			  0x64, 0x20, 0x88, 0x88, 0x88, 0x88, 0x88, 0x88,
+			  0x02, 0x88, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
+			  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETGIP2,
+			  0x02, 0x21, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
+			  0x00, 0x00, 0x00, 0x00, 0x02, 0x46, 0x02, 0x88,
+			  0x88, 0x88, 0x88, 0x88, 0x88, 0x64, 0x88, 0x13,
+			  0x57, 0x13, 0x88, 0x88, 0x88, 0x88, 0x88, 0x88,
+			  0x75, 0x88, 0x23, 0x14, 0x00, 0x00, 0x02, 0x00,
+			  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
+			  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x03, 0x0A,
+			  0xA5, 0x00, 0x00, 0x00, 0x00);
+	dsi_dcs_write_seq(dsi, ST7703_CMD_SETGAMMA,
+			  0x00, 0x09, 0x0D, 0x23, 0x27, 0x3C, 0x41, 0x35,
+			  0x07, 0x0D, 0x0E, 0x12, 0x13, 0x10, 0x12, 0x12,
+			  0x18, 0x00, 0x09, 0x0D, 0x23, 0x27, 0x3C, 0x41,
+			  0x35, 0x07, 0x0D, 0x0E, 0x12, 0x13, 0x10, 0x12,
+			  0x12, 0x18);
+	msleep(20);
+
+	ret = mipi_dsi_dcs_exit_sleep_mode(dsi);
+	if (ret < 0) {
+		DRM_DEV_ERROR(dev, "Failed to exit sleep mode\n");
+		return ret;
+	}
+	msleep(250);
+
+	ret = mipi_dsi_dcs_set_display_on(dsi);
+	if (ret)
+		return ret;
+	msleep(50);
+
+	DRM_DEV_DEBUG_DRIVER(dev, "Panel init sequence done\n");
+	return 0;
+}
+
+static int xbd599_prepare(struct drm_panel *panel)
+{
+	struct xbd599 *ctx = panel_to_xbd599(panel);
+	int ret;
+
+	if (ctx->prepared)
+		return 0;
+
+	ret = regulator_bulk_enable(ARRAY_SIZE(ctx->supplies), ctx->supplies);
+	if (ret)
+		return ret;
+
+	DRM_DEV_DEBUG_DRIVER(ctx->dev, "Resetting the panel\n");
+	gpiod_set_value_cansleep(ctx->reset_gpio, 1);
+	usleep_range(20, 40);
+	gpiod_set_value_cansleep(ctx->reset_gpio, 0);
+	msleep(20);
+
+	ctx->prepared = true;
+
+	return 0;
+}
+
+static int xbd599_enable(struct drm_panel *panel)
+{
+	struct xbd599 *ctx = panel_to_xbd599(panel);
+	int ret;
+
+	ret = xbd599_init_sequence(ctx);
+	if (ret < 0) {
+		DRM_DEV_ERROR(ctx->dev, "Panel init sequence failed: %d\n",
+			      ret);
+		return ret;
+	}
+
+	return 0;
+}
+
+static int xbd599_disable(struct drm_panel *panel)
+{
+	struct xbd599 *ctx = panel_to_xbd599(panel);
+	struct mipi_dsi_device *dsi = to_mipi_dsi_device(ctx->dev);
+
+	return mipi_dsi_dcs_set_display_off(dsi);
+}
+
+static int xbd599_unprepare(struct drm_panel *panel)
+{
+	struct xbd599 *ctx = panel_to_xbd599(panel);
+
+	if (!ctx->prepared)
+		return 0;
+
+	gpiod_set_value_cansleep(ctx->reset_gpio, 1);
+	regulator_bulk_disable(ARRAY_SIZE(ctx->supplies), ctx->supplies);
+	ctx->prepared = false;
+
+	return 0;
+}
+
+static const struct drm_display_mode xbd599_default_mode = {
+	.hdisplay    = 720,
+	.hsync_start = 720 + 40,
+	.hsync_end   = 720 + 40 + 40,
+	.htotal	     = 720 + 40 + 40 + 40,
+	.vdisplay    = 1440,
+	.vsync_start = 1440 + 18,
+	.vsync_end   = 1440 + 18 + 10,
+	.vtotal	     = 1440 + 18 + 10 + 17,
+	.vrefresh    = 60,
+	.clock	     = 69000,
+	.flags	     = DRM_MODE_FLAG_NHSYNC | DRM_MODE_FLAG_NVSYNC,
+
+	.width_mm    = 68,
+	.height_mm   = 136,
+	.type        = DRM_MODE_TYPE_DRIVER | DRM_MODE_TYPE_PREFERRED,
+};
+
+static int xbd599_get_modes(struct drm_panel *panel,
+			    struct drm_connector *connector)
+{
+	struct xbd599 *ctx = panel_to_xbd599(panel);
+	struct drm_display_mode *mode;
+
+	mode = drm_mode_duplicate(connector->dev, &xbd599_default_mode);
+	if (!mode) {
+		DRM_DEV_ERROR(ctx->dev, "Failed to add mode\n");
+		return -ENOMEM;
+	}
+
+	drm_mode_set_name(mode);
+
+	mode->type = DRM_MODE_TYPE_DRIVER | DRM_MODE_TYPE_PREFERRED;
+	connector->display_info.width_mm = mode->width_mm;
+	connector->display_info.height_mm = mode->height_mm;
+	drm_mode_probed_add(connector, mode);
+
+	return 1;
+}
+
+static const struct drm_panel_funcs xbd599_drm_funcs = {
+	.prepare   = xbd599_prepare,
+	.enable    = xbd599_enable,
+	.disable   = xbd599_disable,
+	.unprepare = xbd599_unprepare,
+	.get_modes = xbd599_get_modes,
+};
+
+static int xbd599_probe(struct mipi_dsi_device *dsi)
+{
+	struct device *dev = &dsi->dev;
+	struct xbd599 *ctx;
+	int i, ret;
+
+	ctx = devm_kzalloc(dev, sizeof(*ctx), GFP_KERNEL);
+	if (!ctx)
+		return -ENOMEM;
+
+	for (i = 0; i < ARRAY_SIZE(ctx->supplies); i++)
+		ctx->supplies[i].supply = regulator_names[i];
+
+	ret = devm_regulator_bulk_get(dev, ARRAY_SIZE(ctx->supplies),
+				      ctx->supplies);
+	if (ret < 0) {
+		DRM_DEV_ERROR(&dsi->dev, "cannot get regulators\n");
+		return ret;
+	}
+
+	ctx->reset_gpio = devm_gpiod_get(dev, "reset", GPIOD_OUT_LOW);
+	if (IS_ERR(ctx->reset_gpio)) {
+		DRM_DEV_ERROR(dev, "cannot get reset gpio\n");
+		return PTR_ERR(ctx->reset_gpio);
+	}
+
+	mipi_dsi_set_drvdata(dsi, ctx);
+
+	ctx->dev = dev;
+
+	dsi->lanes = 4;
+	dsi->format = MIPI_DSI_FMT_RGB888;
+	dsi->mode_flags = MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_SYNC_PULSE;
+
+	drm_panel_init(&ctx->panel, &dsi->dev, &xbd599_drm_funcs,
+		       DRM_MODE_CONNECTOR_DSI);
+
+	ret = drm_panel_of_backlight(&ctx->panel);
+	if (ret)
+		return ret;
+
+	drm_panel_add(&ctx->panel);
+
+	ret = mipi_dsi_attach(dsi);
+	if (ret < 0) {
+		DRM_DEV_ERROR(dev, "mipi_dsi_attach failed. Is host ready?\n");
+		drm_panel_remove(&ctx->panel);
+		return ret;
+	}
+
+	DRM_DEV_INFO(dev, "%ux%u@%u %ubpp dsi %udl - ready\n",
+		     xbd599_default_mode.hdisplay,
+		     xbd599_default_mode.vdisplay,
+		     xbd599_default_mode.vrefresh,
+		     mipi_dsi_pixel_format_to_bpp(dsi->format), dsi->lanes);
+
+	return 0;
+}
+
+static void xbd599_shutdown(struct mipi_dsi_device *dsi)
+{
+	struct xbd599 *ctx = mipi_dsi_get_drvdata(dsi);
+	int ret;
+
+	ret = drm_panel_unprepare(&ctx->panel);
+	if (ret < 0)
+		DRM_DEV_ERROR(&dsi->dev, "Failed to unprepare panel: %d\n",
+			      ret);
+}
+
+static int xbd599_remove(struct mipi_dsi_device *dsi)
+{
+	struct xbd599 *ctx = mipi_dsi_get_drvdata(dsi);
+	int ret;
+
+	xbd599_shutdown(dsi);
+
+	ret = mipi_dsi_detach(dsi);
+	if (ret < 0)
+		DRM_DEV_ERROR(&dsi->dev, "Failed to detach from DSI host: %d\n",
+			      ret);
+
+	drm_panel_remove(&ctx->panel);
+
+	return 0;
+}
+
+static const struct of_device_id xbd599_of_match[] = {
+	{ .compatible = "xingbangda,xbd599", },
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, xbd599_of_match);
+
+static struct mipi_dsi_driver xbd599_driver = {
+	.probe	= xbd599_probe,
+	.remove = xbd599_remove,
+	.shutdown = xbd599_shutdown,
+	.driver = {
+		.name = "panel-xingbangda-xbd599",
+		.of_match_table = xbd599_of_match,
+	},
+};
+module_mipi_dsi_driver(xbd599_driver);
+
+MODULE_AUTHOR("Icenowy Zheng <icenowy@aosc.io>");
+MODULE_DESCRIPTION("DRM driver for Xingbangda XBD599 MIPI DSI panel");
+MODULE_LICENSE("GPL v2");
-- 
2.26.2

