From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Mon, 16 Mar 2020 21:35:00 +0800
Subject: [PATCH] dt-bindings: panel: add binding for Xingbangda XBD599 panel

Xingbangda XBD599 is a 5.99" 720x1440 MIPI-DSI LCD panel.

Add its device tree binding.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 .../display/panel/xingbangda,xbd599.yaml      | 50 +++++++++++++++++++
 1 file changed, 50 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/display/panel/xingbangda,xbd599.yaml

diff --git a/Documentation/devicetree/bindings/display/panel/xingbangda,xbd599.yaml b/Documentation/devicetree/bindings/display/panel/xingbangda,xbd599.yaml
new file mode 100644
index 000000000000..b27bcf11198f
--- /dev/null
+++ b/Documentation/devicetree/bindings/display/panel/xingbangda,xbd599.yaml
@@ -0,0 +1,50 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/display/panel/xingbangda,xbd599.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Xingbangda XBD599 5.99in MIPI-DSI LCD panel
+
+maintainers:
+  - Icenowy Zheng <icenowy@aosc.io>
+
+allOf:
+  - $ref: panel-common.yaml#
+
+properties:
+  compatible:
+    const: xingbangda,xbd599
+  reg: true
+  backlight: true
+  reset-gpios: true
+  vcc-supply:
+    description: regulator that supplies the VCC voltage
+  iovcc-supply:
+    description: regulator that supplies the IOVCC voltage
+
+required:
+  - compatible
+  - reg
+  - backlight
+  - vcc-supply
+  - iovcc-supply
+
+additionalProperties: false
+
+examples:
+  - |
+    dsi {
+        #address-cells = <1>;
+        #size-cells = <0>;
+
+        panel@0 {
+            compatible = "xingbangda,xbd599";
+            reg = <0>;
+            backlight = <&backlight>;
+            iovcc-supply = <&reg_dldo2>;
+            vcc-supply = <&reg_ldo_io0>;
+        };
+    };
+
+...
-- 
2.26.2

