From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Peter Robinson <pbrobinson@gmail.com>
Date: Thu, 3 May 2012 20:27:11 +0100
Subject: [PATCH] ARM: tegra: usb no reset

Patch for disconnect issues with storage attached to a
 tegra-ehci controller
---
 drivers/usb/core/hub.c | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/drivers/usb/core/hub.c b/drivers/usb/core/hub.c
index 5b768b80d1ee..6929b6b5186b 100644
--- a/drivers/usb/core/hub.c
+++ b/drivers/usb/core/hub.c
@@ -5517,6 +5517,13 @@ static void hub_event(struct work_struct *work)
 			(u16) hub->change_bits[0],
 			(u16) hub->event_bits[0]);

+	/* Don't disconnect USB-SATA on TrimSlice */
+	if (strcmp(dev_name(hdev->bus->controller), "tegra-ehci.0") == 0) {
+		if ((hdev->state == 7) && (hub->change_bits[0] == 0) &&
+				(hub->event_bits[0] == 0x2))
+			hub->event_bits[0] = 0;
+	}
+
 	/* Lock the device, then check to see if we were
 	 * disconnected while waiting for the lock to succeed. */
 	usb_lock_device(hdev);
-- 
2.26.2

