From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Robert Richter <rrichter@redhat.com>
Date: Thu, 7 Jun 2018 22:59:32 -0400
Subject: [PATCH] Vulcan: AHCI PCI bar fix for Broadcom Vulcan early silicon

Message-id: <1528412373-19128-2-git-send-email-rrichter@redhat.com>
Patchwork-id: 220950
O-Subject: [RHEL-8.0 BZ 1563590 v2 1/2] PCI: Vulcan: AHCI PCI bar fix for Broadcom Vulcan early silicon
Bugzilla: 1563590
RH-Acked-by: Dean Nelson <dnelson@redhat.com>
RH-Acked-by: Mark Langsdorf <mlangsdo@redhat.com>
RH-Acked-by: Mark Salter <msalter@redhat.com>

From: Ashok Kumar Sekar <asekar@redhat.com>

PCI BAR 5 is not setup correctly for the on-board AHCI
controller on Broadcom's Vulcan processor. Added a quirk to fix BAR 5
by using BAR 4's resources which are populated correctly but NOT used
by the AHCI controller actually.

RHEL-only:

Both patches are in RHEL-7.6 also. Inclusion of the patches into RHEL-8
was discussed. Since there are partners with Ax system configurations it
was decided to carry them in RHEL8 too. See:

 https://bugzilla.redhat.com/show_bug.cgi?id=1563590#c1

Upstream Status: RHEL only
Signed-off-by: Ashok Kumar Sekar <asekar@redhat.com>
Signed-off-by: Jayachandran C <jchandra@broadcom.com>
Signed-off-by: Robert Richter <rrichter@redhat.com>
Signed-off-by: Herton R. Krzesinski <herton@redhat.com>
---
 drivers/pci/quirks.c | 24 ++++++++++++++++++++++++
 1 file changed, 24 insertions(+)

diff --git a/drivers/pci/quirks.c b/drivers/pci/quirks.c
index 2a589b6d6ed8..a2b2333e6ab1 100644
--- a/drivers/pci/quirks.c
+++ b/drivers/pci/quirks.c
@@ -4196,6 +4196,30 @@ DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_BROADCOM, 0x9000,
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_BROADCOM, 0x9084,
 				quirk_bridge_cavm_thrx2_pcie_root);

+/*
+ * PCI BAR 5 is not setup correctly for the on-board AHCI controller
+ * on Broadcom's Vulcan processor. Added a quirk to fix BAR 5 by
+ * using BAR 4's resources which are populated correctly and NOT
+ * actually used by the AHCI controller.
+ */
+static void quirk_fix_vulcan_ahci_bars(struct pci_dev *dev)
+{
+	struct resource *r =  &dev->resource[4];
+
+	if (!(r->flags & IORESOURCE_MEM) || (r->start == 0))
+		return;
+
+	/* Set BAR5 resource to BAR4 */
+	dev->resource[5] = *r;
+
+	/* Update BAR5 in pci config space */
+	pci_write_config_dword(dev, PCI_BASE_ADDRESS_5, r->start);
+
+	/* Clear BAR4's resource */
+	memset(r, 0, sizeof(*r));
+}
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_BROADCOM, 0x9027, quirk_fix_vulcan_ahci_bars);
+
 /*
  * Intersil/Techwell TW686[4589]-based video capture cards have an empty (zero)
  * class code.  Fix it.
-- 
2.26.2

