From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Jeremy Cline <jcline@redhat.com>
Date: Thu, 2 Jan 2020 14:24:36 -0500
Subject: [PATCH] mpt*: remove certain deprecated pci-ids

Message-id: <20190708192032.20922-1-jcline@redhat.com>
Patchwork-id: 266421
O-Subject: [ARK INTERNAL PATCH] mpt*: remove certain deprecated pci-ids
Bugzilla:
RH-Acked-by: Don Zickus <dzickus@redhat.com>
RH-Acked-by: Jarod Wilson <jarod@redhat.com>

Commit 8f8384503e40 ("scsi: mpt3sas: Add support for NVMe Switch
Adapter") introduced a new PCI device ID which broke the patch context.

    Message-id: <20180403143030.4971-1-thenzl@redhat.com>
    Patchwork-id: 7431
    O-Subject: [kernel team] [RHEL8 e-stor PATCH] mpt*: remove certain deprecated pci-ids
    Bugzilla: 1511953
    RH-Acked-by: Maurizio Lombardi <mlombard@redhat.com>
    RH-Acked-by: Chris Leech <cleech@redhat.com>

    bz#1511953
    brew - task_15594743

    RH specific - remove EOL devices from the pci-id table
    (devices to remove were selected by Broadcom)

    Signed-off-by: Herton R. Krzesinski <herton@redhat.com>

Upstream Status: RHEL only
Signed-off-by: Jeremy Cline <jcline@redhat.com>
---
 drivers/scsi/mpt3sas/mpt3sas_scsih.c | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/drivers/scsi/mpt3sas/mpt3sas_scsih.c b/drivers/scsi/mpt3sas/mpt3sas_scsih.c
index 2e2756d8a49b..a67a47d3fce1 100644
--- a/drivers/scsi/mpt3sas/mpt3sas_scsih.c
+++ b/drivers/scsi/mpt3sas/mpt3sas_scsih.c
@@ -11033,6 +11033,7 @@ bool scsih_ncq_prio_supp(struct scsi_device *sdev)
  * The pci device ids are defined in mpi/mpi2_cnfg.h.
  */
 static const struct pci_device_id mpt3sas_pci_table[] = {
+#ifndef CONFIG_RHEL_DIFFERENCES
 	/* Spitfire ~ 2004 */
 	{ MPI2_MFGPAGE_VENDORID_LSI, MPI2_MFGPAGE_DEVID_SAS2004,
 		PCI_ANY_ID, PCI_ANY_ID },
@@ -11051,6 +11052,7 @@ static const struct pci_device_id mpt3sas_pci_table[] = {
 		PCI_ANY_ID, PCI_ANY_ID },
 	{ MPI2_MFGPAGE_VENDORID_LSI, MPI2_MFGPAGE_DEVID_SAS2116_2,
 		PCI_ANY_ID, PCI_ANY_ID },
+#endif
 	/* Thunderbolt ~ 2208 */
 	{ MPI2_MFGPAGE_VENDORID_LSI, MPI2_MFGPAGE_DEVID_SAS2208_1,
 		PCI_ANY_ID, PCI_ANY_ID },
@@ -11075,9 +11077,11 @@ static const struct pci_device_id mpt3sas_pci_table[] = {
 		PCI_ANY_ID, PCI_ANY_ID },
 	{ MPI2_MFGPAGE_VENDORID_LSI, MPI2_MFGPAGE_DEVID_SWITCH_MPI_EP_1,
 		PCI_ANY_ID, PCI_ANY_ID },
+#ifndef CONFIG_RHEL_DIFFERENCES
 	/* SSS6200 */
 	{ MPI2_MFGPAGE_VENDORID_LSI, MPI2_MFGPAGE_DEVID_SSS6200,
 		PCI_ANY_ID, PCI_ANY_ID },
+#endif
 	/* Fury ~ 3004 and 3008 */
 	{ MPI2_MFGPAGE_VENDORID_LSI, MPI25_MFGPAGE_DEVID_SAS3004,
 		PCI_ANY_ID, PCI_ANY_ID },
-- 
2.26.2

